===============================================================================
Please read before using.

                                 Copyright CANON FINETECH NISCA INC. 2015-2023
===============================================================================


-------------------------------------------------------------------------------

- Contents -

    1. Introduction
    2. Copyright Notices
    3. CFT Network Operating Environment
    4. Precautions for CFT Network


-------------------------------------------------------------------------------

1. Introduction
  This product is a network communication software that supports
  Microsoft(R) Windows(R) 10  (hereafter Windows).
  This product is required for the network communication with the
  CANON FINETECH NISCA INC. printer.

-------------------------------------------------------------------------------

2. Copyright Notices
  Microsoft, Windows are registered trademarks of the Microsoft Corporation in
  the United States and other countries.
  Other company names and brand names may be registered trademarks
  or trademarks of their respective companies.

-------------------------------------------------------------------------------

3. CFT Network Operating Environment

   "Software"
   
    Windows 10 (x86)

   "Hardware"

     Computer:
      Computer that is guaranteed for the operation of the OS
      Intel processor, or other compatible microprocessor with
      a Gigabit Ethernet(10/100/1000Mbps) network interface

     Memory:
        Sufficient capacity guaranteed to operate with Windows.

     Hard disk:
        Requires capacity of 50 MB (or more) at installation
        of printer driver.

     Printer
        Swiftcolor SCC-4000D

-------------------------------------------------------------------------------

4. Precautions for CFT Network

   "Matters to note when printing with a 10Mbps network interface"
        You may fail to print when printing in a 10Mbps network interface for
        CFT Network. To print with a 10Mbps network interface, start the network
        utility, select "Environment settings" "Timeout settings", and check
        "Extend timeout value".

-------------------------------------------------------------------------------


